



**Aluminum Raised Floor**





**Abeite** Aluminum Raised Floor made from precision machined die-cast aluminum,

specifically designed for the ultra-clean environment. The surface of the floor can be

epoxy powdered or nickel-cadmium plated according to the needs. The top finished

with HPL/PVC/Ceramic, etc covering, aluminum panel is available with corner locking

for vibration control.


|  |  |
| --- | --- |
| Type: | FS662-2000 |
| Finished Floor Height: | 100-2000mm |
| Panel Size: | 600\*600mm |
| Panel Thickness: | Solid Panel / Perforated panel |
| Finish Covering: | 1.0-2.0mm Anti-static Laminate HPL、2.0-3.0mm PVC、10mm Cermic、Marble、Granite、Nature Wood and etc. |
| Edge trim: | Trimless / Nomal trim, |
| Corner lock hole | With / Without |
| Installation: | With Stringer System |




**Characteristics:**

* 100% recyclable
* Novel structural design, high dimensional accuracy, not easy to deform
* Lightweight, high density, high strength, high load capacity
* Waterproof, fireproof, anti-corrosion, anti-magnetic, no pollution, no radiation
* Performance and its stability and never decline good static conductivity



****


****

**Applications:**

Aluminum panel is mainly used for laying clean rooms with high requirements on air cleanliness, such as semiconductor production workshops,hospital laboratories, etc.

**Ventilation Rate 15%**





**Ventilation Rate 60% Ventilation Rate 55%**





Changzhou Abeite Computer Room Equipment Co.,Ltd

Add: No. 108, Chaoyang Village, Hengshanqiao Town, Wujin District,

Changzhou City, Jiangsu Province，China

Tel: +86(519)86056270

Fax: +86(519)86056270

E-mail: info@abeiteraisedfloor.com

Web: www. abeiteraisedfloor.com